|  |  |
| --- | --- |
| PTHG-MTRA new system: VISION – Snapshots:    * MENU3 – new snapshot:   + ARTEsnp & NSOAsnp added at the bottom | Present system: VISION – Snapshots:  * MENU3 – present snapshot: |
| * ARTEsnp – new snapshot:   + ARTE system status information. |  |
| * NSOAsnp – new snapshot:   + List of the Terminals with No SIGN-ON On ARTE system. |  |
| * SYSsnp – modified snapshot:   + ARTE PASS> line added.   + \*SUPPTH parameter added.     - SUPPress Pass THru [0=enabled/1=disabled].   + \*MAXPTH parameter added.     - MAXimum of Pass THru outstanding transactions.   + INARTE counter added.     - Balance between transactions sent and received from ARTE system. | * SYSsnp – present snapshot:   + \*SUPINs parameter removed.     - Replaced with \*SUPPTH new parameter. |
| * AGTsnp – modified snapshot:   + \*AGTPTH parameter added below REDMIN.     - Suppress Pass THru at agent level [0=enabled/1=disabled]. | * AGTsnp – present snapshot: |